{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["表-08 分部分项工程和单价措施项目清单与计价表"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"表-08 分部分项工程和单价措施项目清单与计价表","index":0,"n_rows":124,"n_cols":11,"rows_kept":124,"merged":[[0,0,0,10],[1,0,1,10],[2,0,2,3],[2,4,2,7],[2,8,2,10],[3,0,5,0],[3,1,5,1],[3,2,5,2],[3,3,5,4],[3,5,5,5],[3,6,5,6],[3,7,3,10],[4,7,5,8],[4,9,5,9],[4,10,5,10],[6,3,6,4],[6,7,6,8],[7,3,7,4],[7,7,7,8],[8,3,8,4],[8,7,8,8],[9,3,9,4],[9,7,9,8],[10,3,10,4],[11,3,11,4],[11,7,11,8],[12,3,12,4],[12,7,12,8],[13,3,13,4],[13,7,13,8],[14,3,14,4],[14,7,14,8],[15,3,15,4],[15,7,15,8],[16,0,16,8],[17,0,17,10],[18,0,18,3],[18,4,18,7],[18,8,18,10],[19,0,19,10],[20,0,20,10],[21,0,21,3],[21,4,21,7],[21,8,21,10],[22,0,24,0],[22,1,24,1],[22,2,24,2],[22,3,24,4],[22,5,24,5],[22,6,24,6],[22,7,22,10],[23,7,24,8],[23,9,24,9],[23,10,24,10],[25,3,25,4],[25,7,25,8],[26,3,26,4],[26,7,26,8],[27,3,27,4],[27,7,27,8],[28,3,28,4],[28,7,28,8],[29,3,29,4],[29,7,29,8],[30,3,30,4],[30,7,30,8],[31,0,31,8],[32,0,32,10],[33,0,33,3],[33,4,33,7],[33,8,33,10],[34,0,34,10],[35,0,35,10],[36,0,36,3],[36,4,36,7],[36,8,36,10],[37,0,39,0],[37,1,39,1],[37,2,39,2],[37,3,39,4],[37,5,39,5],[37,6,39,6],[37,7,37,10],[38,7,39,8],[38,9,39,9],[38,10,39,10],[40,3,40,4],[40,7,40,8],[41,3,41,4],[41,7,41,8],[42,3,42,4],[42,7,42,8],[43,3,43,4],[43,7,43,8],[44,3,44,4],[44,7,44,8],[45,3,45,4],[45,7,45,8],[46,3,46,4],[46,7,46,8],[47,0,47,8],[48,0,48,10],[49,0,49,3],[49,4,49,7],[49,8,49,10],[50,0,50,10],[51,0,51,10],[52,0,52,3],[52,4,52,7],[52,8,52,10],[53,0,55,0],[53,1,55,1],[53,2,55,2],[53,3,55,4],[53,5,55,5],[53,6,55,6],[53,7,53,10],[54,7,55,8],[54,9,55,9],[54,10,55,10],[56,3,56,4],[56,7,56,8],[57,3,57,4],[57,7,57,8],[58,3,58,4],[59,3,59,4],[59,7,59,8],[60,0,60,8],[61,0,61,10],[62,0,62,3],[62,4,62,7],[62,8,62,10],[63,0,63,10],[64,0,64,10],[65,0,65,3],[65,4,65,7],[65,8,65,10],[66,0,68,0],[66,1,68,1],[66,2,68,2],[66,3,68,4],[66,5,68,5],[66,6,68,6],[66,7,66,10],[67,7,68,8],[67,9,68,9],[67,10,68,10],[69,3,69,4],[69,7,69,8],[70,3,70,4],[70,7,70,8],[71,3,71,4],[71,7,71,8],[72,3,72,4],[72,7,72,8],[73,3,73,4],[73,7,73,8],[74,3,74,4],[74,7,74,8],[75,3,75,4],[75,7,75,8],[76,0,76,8],[77,0,77,10],[78,0,78,3],[78,4,78,7],[78,8,78,10],[79,0,79,10],[80,0,80,10],[81,0,81,3],[81,4,81,7],[81,8,81,10],[82,0,84,0],[82,1,84,1],[82,2,84,2],[82,3,84,4],[82,5,84,5],[82,6,84,6],[82,7,82,10],[83,7,84,8],[83,9,84,9],[83,10,84,10],[85,3,85,4],[85,7,85,8],[86,3,86,4],[86,7,86,8],[87,3,87,4],[87,7,87,8],[88,3,88,4],[88,7,88,8],[89,0,89,8],[90,0,90,10],[91,0,91,3],[91,4,91,7],[91,8,91,10],[92,0,92,10],[93,0,93,10],[94,0,94,3],[94,4,94,7],[94,8,94,10],[95,0,97,0],[95,1,97,1],[95,2,97,2],[95,3,97,4],[95,5,97,5],[95,6,97,6],[95,7,95,10],[96,7,97,8],[96,9,97,9],[96,10,97,10],[98,3,98,4],[98,7,98,8],[99,3,99,4],[99,7,99,8],[100,3,100,4],[100,7,100,8],[101,3,101,4],[101,7,101,8],[102,0,102,8],[103,0,103,10],[104,0,104,3],[104,4,104,7],[104,8,104,10],[105,0,105,10],[106,0,106,10],[107,0,107,3],[107,4,107,7],[107,8,107,10],[108,0,110,0],[108,1,110,1],[108,2,110,2],[108,3,110,4],[108,5,110,5],[108,6,110,6],[108,7,108,10],[109,7,110,8],[109,9,110,9],[109,10,110,10],[111,3,111,4],[111,7,111,8],[112,3,112,4],[112,7,112,8],[113,3,113,4],[113,7,113,8],[114,3,114,4],[114,7,114,8],[115,3,115,4],[115,7,115,8],[116,3,116,4],[116,7,116,8],[117,3,117,4],[117,7,117,8],[118,3,118,4],[118,7,118,8],[119,3,119,4],[119,7,119,8],[120,0,120,8],[121,0,121,8],[122,0,122,10],[123,0,123,3],[123,4,123,7],[123,8,123,10]],"flags":["formulas_cached_only"]}
["","","","","","","","","","",""]
["工程量清单报价表",null,"","","","","","","","",""]
["工程名称：甘德尔河景观绿化工程","","","",null,"","","","第  1  页  共  8  页","",""]
["序号","项目编码","项目名称","项 目 特 征","","计量单位","工程量","金额（元）","","",""]
["","","","","","","","综合单价（含税金)","","合价","备注"]
["","","","","","","","","",""]
["","","平台","","","","","","","",""]
[1,"010606006001","木平台做法一","1、100厚c15混凝土垫层\n2、预埋件\n3、100*60*5镀锌方管龙骨\n4、L*140*40塑木平台面层缝宽5mm自攻钉固定（主材甲供）\n5、详细做法见施工图(木平台做法变更图剖面大样图）","","m2",1412,"","",null,""]
[2,"010606006002","木平台做法二","1.素土夯实\n2.300厚天然级配砂砾人工夯实\n3.C20混凝土基础\n4.预埋铁件M-1\n5.镀锌方钢管100*60*5龙骨安装\n6.侧板L100*40塑木（主材甲供）\n7.L140*40塑木平台面层  缝宽5mm（主材甲供）\n8.详细做法见施工图(木平台做法XS-03)","","m2",500,"","","",""]
[null,null,"塑木坐凳","1、410*80*80方形防腐木立柱安装与两根240*80*80方形防腐木（榫卯粘接）与塑木地板两根Ø10螺栓固定（主材甲供）\n2、L140*40塑木凳面  缝宽10mm木螺丝固定（主材甲供）\n3、详细做法见施工图木（平台做法XS-06）",null,"m",50]
[null,null,"塑木栏杆","1、内口径100*100*6钢套筒与主龙骨焊接\n2、1040*100*100方形塑木立柱两根Ø10螺栓与钢套筒固定（主材甲供）\n3、三根Ø25棕绳与立柱固定\n4、详细做法见施工图(木平台做法XS-03)",null,"m",500]
["","","分部小计","","","","","","","",""]
["","","广场铺装","","","","","","","",""]
[3,"011102003001","青石板错缝铺（1000*500*50）","1、100厚c15混凝土垫层\r\n2、50厚1：3干硬性水泥砂浆\r\n3、3-5厚素水泥浆\r\n4、青石板错缝铺（1000*500*50）（主材甲供）","","m2",197,"","","",""]
[4,"011106003001","30厚黄金麻火烧面花岗岩冰裂纹碎拼","1、100厚c15混凝土垫层\r\n2、50厚1：3干硬性水泥砂浆\r\n3、3-5厚素水泥浆\r\n4、30厚火烧面黄金麻火烧面花岗岩冰裂纹碎拼（主材甲供）","","m2",500,"","","",""]
[5,"011102003002","蒙古黑光面花岗岩（600*400*50）","1、100厚c15混凝土垫层\r\n2、50厚1：3干硬性水泥砂浆\r\n3、3-5厚素水泥浆\r\n4、蒙古黑光面花岗岩（600*400*50）（主材甲供）","","m2",400,"","","",""]
["本页小计","","","","","","","","","",""]
["注：为计取规费等的使用，可在表中增设其中：“定额人工费”。","","","","","","","","","",""]
["","","","","","","","","表-08","",""]
["","","","","","","","","","",""]
["工程量清单报价表",null,"","","","","","","","",""]
["工程名称：甘德尔河景观绿化工程","","","",null,"","","","第  2  页  共  8  页","",""]
["序号","项目编码","项目名称","项 目 特 征","","计量单位","工程量","金额（元）","","",""]
["","","","","","","","综合单价（含税金)","","合价","备注"]
["","","","","","","","","",""]
[6,"011102003003","蒙古黑光面花岗岩（400*200*30）","1、100厚c15混凝土垫层\r\n2、50厚1：3干硬性水泥砂浆\r\n3、3-5厚素水泥浆\r\n4、蒙古黑光面花岗岩（400*200*30）（主材甲供）","","m2",60,"","","",""]
[7,"011102003004","蒙古黑火烧面花岗岩（800*500*50）","1、100厚c15混凝土垫层\r\n2、50厚1：3干硬性水泥砂浆\r\n3、3-5厚素水泥浆\r\n4、蒙古黑火烧面花岗岩（800*500*50）（主材甲供）","","m2",214,"","","",""]
[8,"011102003005","蒙古黑火烧面花岗岩（800*400*50）","1、100厚c15混凝土垫层\r\n2、50厚1：3干硬性水泥砂浆\r\n3、3-5厚素水泥浆\r\n4、蒙古黑火烧面花岗岩（800*400*50）（主材甲供）","","m2",400,"","","",""]
[9,"011102003006","黄金麻火烧面花岗岩（400*400*30）","1、100厚c15混凝土垫层\r\n2、50厚1：3干硬性水泥砂浆\r\n3、3-5厚素水泥浆\r\n4、黄金麻火烧面花岗岩（400*400*30）（主材甲供）","","m2",4200,"","","",""]
[10,"011102003007","蒙古黑光面花岗岩（800*300*50）","1、100厚c15混凝土垫层\r\n2、50厚1：3干硬性水泥砂浆\r\n3、3-5厚素水泥浆\r\n4、蒙古黑光面花岗岩（800*300*50）（主材甲供）","","m2",110,"","","",""]
[11,"011102003008","蒙古黑光面花岗岩（800*200*50）","1、100厚c15混凝土垫层\r\n2、50厚1：3干硬性水泥砂浆\r\n3、3-5厚素水泥浆\r\n4、蒙古黑光面花岗岩（800*200*50）（主材甲供）","","m2",48,"","","",""]
["本页小计","","","","","","","","","",""]
["注：为计取规费等的使用，可在表中增设其中：“定额人工费”。","","","","","","","","","",""]
["","","","","","","","","表-08","",""]
["","","","","","","","","","",""]
["工程量清单报价表",null,"","","","","","","","",""]
["工程名称：甘德尔河景观绿化工程","","","",null,"","","","第  3  页  共  8  页","",""]
["序号","项目编码","项目名称","项 目 特 征","","计量单位","工程量","金额（元）","","",""]
["","","","","","","","综合单价（含税金)","","合价","备注"]
["","","","","","","","","",""]
[12,"011102003009","芝麻灰火烧面花岗岩（400*400*30）","1、100厚c15混凝土垫层\r\n2、50厚1：3干硬性水泥砂浆\r\n3、3-5厚素水泥浆\r\n4、芝麻灰火烧面花岗岩（400*400*30）（主材甲供）","","m2",700,"","","",""]
[13,"011102003010","黄金麻火烧面花岗岩（400*400*30）","1、100厚c15混凝土垫层\r\n2、50厚1：3干硬性水泥砂浆\r\n3、3-5厚素水泥浆\r\n4、黄金麻火烧面花岗岩（400*400*30）（主材甲供）","","m2",4000,"","","",""]
[14,"050201004001","树池芝麻灰光面花岗岩（650*350*280）","1、100厚c15混凝土垫层\r\n2、50厚1：3干硬性水泥砂浆\r\n3、树池芝麻灰光面花岗岩（650*350*280）（主材甲供）","","m",7.8,"","","",""]
[15,"050201004002","树池芝麻灰光面花岗岩（350*350*280）","1、100厚c15混凝土垫层\r\n2、50厚1：3干硬性水泥砂浆\r\n3、树池芝麻灰光面花岗岩（350*350*280）（主材甲供）","","m",4.2,"","","",""]
[16,"011107002001","芝麻灰自然面条石坐凳（6000*500*450）","1、100厚c15混凝土垫层\r\n2、50厚1：3干硬性水泥砂浆\r\n3、芝麻灰自然面条石坐凳（6000*500*450）","","m2",51,"","","",""]
[17,"011102003011","黄金麻火烧面花岗岩（500*300*30）","1、100厚c15混凝土垫层\r\n2、50厚1：3干硬性水泥砂浆\r\n3、3-5厚素水泥浆\r\n4、黄金麻火烧面花岗岩（500*300*30）（主材甲供）","","m2",100,"","","",""]
[18,"011102003012","新型陶瓷砖（230*115*20）","1、100厚c15混凝土垫层\r\n2、50厚1：3干硬性水泥砂浆\r\n3、10厚素水泥浆\r\n4、新型陶瓷砖（230*115*20）（主材甲供）","","m2",4500,"","","",""]
["本页小计","","","","","","","","","",""]
[]
["","","","","","","","","表-08","",""]
["","","","","","","","","","",""]
["工程量清单报价表",null,"","","","","","","","",""]
["工程名称：甘德尔河景观绿化工程","","","",null,"","","","第  4  页  共  8  页","",""]
["序号","项目编码","项目名称","项 目 特 征","","计量单位","工程量","金额（元）","","",""]
["","","","","","","","综合单价（含税金)","","合价","备注"]
["","","","","","","","","",""]
[19,"011107002002","500宽挡墙坐凳","1、机械开槽760mm*500mm人工装车三轮车倒运，运距500m以内\n2、人工素土夯实（密实度94%）\n3、760*300厚天然级配砂砾人工夯实（密实度95%）\n4、支模浇筑560*200c20混凝土基础\n5、支模浇筑360*600c20混凝土基础\n6、详见施工图（铺装做法图XS-29）","","m",3100,"","","",""]
[20,"011107002003","300宽挡墙一","1、机械开槽600mm*500mm人工装车三轮车倒运，运距500m以内\n2、人工素土夯实（密实度94%）\n3、600*300厚天然级配砂砾人工夯实（密实度95%）\n4、支模浇筑400*200c20混凝土基础\n5、支模浇筑200*650c20混凝土基础\n6、详见施工图（铺装做法图XS-29）","","m",750,"","","",""]
[20,"011107002003","300宽挡墙二","1、机械开槽600mm*500mm人工装车三轮车倒运，运距500m以内\n2、人工素土夯实（密实度94%）\n3、600*300厚天然级配砂砾人工夯实（密实度95%）\n4、支模浇筑400*200c20混凝土基础\n5、支模浇筑200*850c20混凝土基础\n6、详见施工图",null,"m",750]
[21,"011107002004","500宽挡墙坐凳","1、机械开槽760mm*500mm人工装车三轮车倒运，运距500m以内\n2、人工素土夯实（密实度94%）\n3、760*300厚天然级配砂砾人工夯实（密实度95%）\n4、弧形支模浇筑560*200c20混凝土基础\n5、弧形支模浇筑360*600c20混凝土基础\n6、详见施工图（铺装做法图XS-29）",null,"m",1500,"","","",""]
["本页小计","","","","","","","","","",""]
["注：为计取规费等的使用，可在表中增设其中：“定额人工费”。","","","","","","","","","",""]
["","","","","","","","","表-08","",""]
["","","","","","","","","","",""]
["工程量清单报价表",null,"","","","","","","","",""]
["工程名称：甘德尔河景观绿化工程","","","",null,"","","","第  5  页  共  8  页","",""]
["序号","项目编码","项目名称","项 目 特 征","","计量单位","工程量","金额（元）","","",""]
["","","","","","","","综合单价（含税金)","","合价","备注"]
["","","","","","","","","",""]
[22,"011107002005","300宽挡墙一","1、机械开槽600mm*500mm人工装车三轮车倒运，运距500m以内\n2、人工素土夯实（密实度94%）\n3、600*300厚天然级配砂砾人工夯实（密实度95%）\n4、弧形支模浇筑400*200c20混凝土基础\n5、弧形支模浇筑200*650c20混凝土基础\n6、详见施工图（铺装做法图XS-29）",null,"m",750,"","","",""]
[null,null,"300宽挡墙二","1、机械开槽600mm*500mm人工装车三轮车倒运，运距500m以内\n2、人工素土夯实（密实度94%）\n3、600*300厚天然级配砂砾人工夯实（密实度95%）\n4、弧形支模浇筑400*200c20混凝土基础\n5、弧形支模浇筑200*850c20混凝土基础\n6、详见施工图（铺装做法图XS-29）",null,"m",750,""]
[null,null,"300宽挡墙三","1、机械开槽800mm*570mm人工装车三轮车倒运，运距500m以内\n2、人工素土夯实（密实度94%）\n3、800*300厚天然级配砂砾人工夯实（密实度95%）\n4、弧形支模浇筑400*600c20混凝土基础\n5、弧形支模浇筑200*1170c20混凝土基础\n6、详见施工图（广场详图ZS-07）",null,"m",750,""]
[23,"011107002006","蒙古黑光面花岗岩压顶R20两侧倒角（600*300*50）","1、30厚1：3水泥砂浆\r\n2、蒙古黑光面花岗岩压顶R20两侧倒角（600*300*50（主材甲供）","","m",2500,"","","",""]
[24,"011107002007","蒙古黑光面花岗岩压顶R20两侧倒角异形（600*300*50）","1、30厚1：3水泥砂浆\r\n2、蒙古黑光面花岗岩压顶R20两侧倒角异形（600*300*50）（主材甲供）","","m",600,"","","",""]
[25,"011102003013","20厚不规则文化石贴面","1、10厚1：3水泥砂浆打底挂纤维网打毛\n2、10厚1：2.5水泥砂浆结合层\n3、20厚不规则文化石贴面（文化石刷水泥素浆，内参107胶，勾凹缝缝宽10厚）主材甲供","","m2",1458.17,"","","",""]
[26,"011102003014","20厚不规则文化石贴面异形","1、10厚1：3水泥砂浆打底挂纤维网打毛\n2、10厚1：2.5水泥砂浆结合层\n3、20厚不规则文化石贴面异形（文化石刷水泥素浆，内参107胶，勾凹缝缝宽10厚）主材甲供","","m2",500,"","","",""]
["本页小计","","","","","","","","","",""]
["注：为计取规费等的使用，可在表中增设其中：“定额人工费”。","","","","","","","","","",""]
["","","","","","","","","表-08","",""]
["","","","","","","","","","",""]
["工程量清单报价表",null,"","","","","","","","",""]
["工程名称：甘德尔河景观绿化工程","","","",null,"","","","第  6  页  共  8  页","",""]
["序号","项目编码","项目名称","项 目 特 征","","计量单位","工程量","金额（元）","","",""]
["","","","","","","","综合单价（含税金)","","合价","备注"]
["","","","","","","","","",""]
[27,"011107002008","蒙古黑火烧面花岗岩压顶R20两侧倒角（600*500*50）","1、30厚1：3水泥砂浆\n2、蒙古黑火烧面花岗岩压顶R20两侧倒角（800*500*50）(主材甲供）","","m",600,"","","",""]
[28,"011107002009","蒙古黑火烧面花岗岩压顶R20两侧倒角异形（600*500*50）","1、30厚1：3水泥砂浆\n2、蒙古黑火烧面花岗岩压顶R20两侧倒角异形（800*500*50）（主材甲供）","","m",400,"","","",""]
[29,"011107002010","石笼坐凳","1、机械开槽960mm*100mm人工装车三轮车倒运，运距500m以内\n2、人工素土夯实（密实度94%）\n3、300厚天然级配砂砾人工夯实（密实度95%）\n4、460mm*480mmc20混凝土基础\n5、4根Ø8钢筋，8厚钢板预埋件\n6、成品40*40*5不锈钢网片与钢板角钢焊接\n7、不锈钢网片内填充145厚80-200卵石（主材甲供）\n8、L*130*40塑木面层（缝宽5mm）（主材甲供）\n9、详见施工图(广场详图1XS-07)","","m",37.1,"","","",""]
[30,"011107002011","塑木坐凳","1、2根Ø10螺栓与240*80*80防腐木（榫卯粘接）固定于木平台上（主材甲供）\n2、两侧采用410*80*80方形防腐木与上下240*80*80防腐木榫卯粘接固定（主材甲供）\n3、面层L*140*40塑木（缝宽10mm）木螺丝固定（主材甲供）\n4、详见施工图","","m",69,"","","",""]
["本页小计","","","","","","","","","",""]
["注：为计取规费等的使用，可在表中增设其中：“定额人工费”。","","","","","","","","","",""]
["","","","","","","","","表-08","",""]
["","","","","","","","","","",""]
["工程量清单报价表",null,"","","","","","","","",""]
["工程名称：甘德尔河景观绿化工程","","","",null,"","","","第  7  页  共  8  页","",""]
["序号","项目编码","项目名称","项 目 特 征","","计量单位","工程量","金额（元）","","",""]
["","","","","","","","综合单价（含税金)","","合价","备注"]
["","","","","","","","","",""]
[31,"010504002001","钢板景墙","1、机械开槽960mm*100mm人工装车三轮车倒运，运距500m以内\n2、人工素土夯实（密实度94%）\n3、300厚天然级配砂砾夯实（密实度95%）\n4、弧形支模浇筑200*680c20混凝土基础\n5、弧形支模浇筑320*480c20混凝土基础下M-1预埋件\n6、10*350钢板用膨胀螺栓与混凝土固定\n7、300宽顶部两侧R15倒角5厚钢板与M-1预埋件焊接\n8、底部100*100两侧填充?30-80杂色机制卵石（主材甲供）\n9、详见施工图(广场详图ZS-07)","","m",23,"","","",""]
["","","分部小计","","","","","","","",""]
["","","台阶","","","","","","","",""]
[32,"011107002012","台阶1","1、机械开槽500mm厚人工装车三轮车倒运，运距500m以内\n2、人工素土夯实（密实度94%）\n3、300厚天然级配砂砾人工夯实（密实度95%）\n4、支模浇筑100mm厚c15混凝土垫层\n5、50厚1：3干硬性水泥砂浆\n6、600*200*180蒙古黑光面花岗岩立板（主材甲供）\n7、400*400*30黄金麻火烧面花岗岩台阶板（主材甲供）\n8、详见施工图(广场详图1XS-06)","","m2",100,"","","",""]
["本页小计","","","","","","","","","",""]
["注：为计取规费等的使用，可在表中增设其中：“定额人工费”。","","","","","","","","","",""]
["","","","","","","","","表-08","",""]
["","","","","","","","","","",""]
["工程量清单报价表",null,"","","","","","","","",""]
["工程名称：甘德尔河景观绿化工程","","","",null,"","","","第  8  页  共  8  页","",""]
["序号","项目编码","项目名称","项 目 特 征","","计量单位","工程量","金额（元）","","",""]
["","","","","","","","综合单价（含税金)","","合价","备注"]
["","","","","","","","","",""]
[33,"011107002013","台阶2","1、机械开槽500mm厚人工装车三轮车倒运，运距500m以内\n2、人工素土夯实（密实度94%）\n3、300厚天然级配砂砾人工夯实（密实度95%）\n4、支模浇筑c15混凝土垫层\n5、50厚1：3干硬性水泥砂浆\n6、800*100*30黄金麻火烧面花岗岩立板（主材甲供）\n7、800*430*50芝麻灰火烧面花岗岩台阶板（主材甲供）\n8、详见施工图(铺装做法图XS-30)","","m2",2000,"","","",""]
[34,"011107002014","台阶3","1、机械开槽500mm厚人工装车三轮车倒运，运距500m以内\n2、人工素土夯实（密实度94%）\n3、300厚天然级配砂砾人工夯实（密实度95%）\n4、支模浇筑c15混凝土垫层\n5、50厚1：3干硬性水泥砂浆\n6、芝麻灰火烧面花岗岩台阶立板600*170*20（主材甲供）\n7、芝麻灰火烧面花岗岩台阶板R15倒角380*600*30（主材甲供）\n8、详见施工图(铺装做法图XS-30)","","m2",3000,"","","",""]
[null,null,"台阶3栏杆","1、M-1预埋件\n2、100*15镀锌钢板立柱与预埋件焊接内穿Ø10镀锌钢丝绳\n3、L*80*5镀锌钢板扶手连接板与镀锌钢板立柱焊接\n4、100*60*L实心塑木扶手（主材甲供）\n5、详见图纸（铺装做法图XS-30)",null,"m",1000]
["","","分部小计","","","","","","","",""]
["","","措施项目","","","","","","","",""]
["","","","","","","","","","",""]
["","","","","","","","","","",""]
["","","","","","","","","","",""]
["","","","","","","","","","",""]
["本页小计","","","","","","","","","",""]
["合计","","","","","","","","","",""]
[]
["","","","","","","","",null,"",""]